[:SENSe]:TDSCdma:TIME:STARt | command/query

Gets or sets the start boundary.

Command Syntax: | [:SENSe]:TDSCdma:TIME:STARt <value>
<value> | ::= | "Subframe" | "TwoFrame"
Query Syntax: | [:SENSe]:TDSCdma:TIME:STARt?
Returns | ::= | "Subframe" | "TwoFrame"
Remarks: | <none>
Example: |
    :TDSC:TIME:STAR "Subframe"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.StartBoundary Agilent.SA.Vsa.Tdscdma.StartBoundaryType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |