[:SENSe]:W11A:PRESet | command

Preset the WLAN 80211 a/g/j/p measurement.

Command Syntax: | [:SENSe]:W11A:PRESet <standard>
<standard> | ::= | "Ieee80211A" | "Hiperlan2" | "Ieee80211GDsssOfdm" | "Ieee80211ATurbo" | "AstmDsrc" | "Ieee80211JHalf"
Remarks: | <none>
Example: |
    :W11A:PRES "Ieee80211A"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211Agjp.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.Wlan80211Agjp.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |