[:SENSe]:WCDMa:CHANnel:DESPread:ULINk:THSDpcch:LOCation | command/query

Gets or sets the tHS-DPCCH code channel location.

Command Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:ULINk:THSDpcch:LOCation <value>
<value> | ::= | "SpreadCodeLength256CodeChannel1I" | "SpreadCodeLength256CodeChannel32Q" | "SpreadCodeLength256CodeChannel33Q" | "SpreadCodeLength256CodeChannel64Q"
Query Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:ULINk:THSDpcch:LOCation?
Returns | ::= | "SpreadCodeLength256CodeChannel1I" | "SpreadCodeLength256CodeChannel32Q" | "SpreadCodeLength256CodeChannel33Q" | "SpreadCodeLength256CodeChannel64Q"
Remarks: | <none>
Example: |
    :WCDM:CHAN:DESP:ULIN:THSD:LOC "SpreadCodeLength256CodeChannel1I"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.ThsdpcchLocation Agilent.SA.Vsa.Wcdma.ThsdpcchLocation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |