[:SENSe]:LTE[:FORMat]:DLINk:CELL:MODE | command/query

Gets or sets the Cell ID Mode as being auto-detected or manually detected (Downlink only).

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:CELL:MODE <value>
<value> | ::= | "Auto" | "Manual"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:CELL:MODE?
Returns | ::= | "Auto" | "Manual"
Remarks: | <none>
Example: |
    :LTE:DLIN:CELL:MODE "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.CellIdMode Agilent.SA.Vsa.Lte.CellIdModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |