[:SENSe]:GSM[:FORMat]:TSCindex | command/query

Gets or sets the TSC index of the time slot to analyze when TSC auto detection is disabled.

Command Syntax: | [:SENSe]:GSM[:FORMat]:TSCindex <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:GSM[:FORMat]:TSCindex?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.GsmEdgeEvolution.Interfaces.MeasurementExtension.TscIndex

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |