[:SENSe]:LTE:PROFile:ULINk:USER:PUCCh:DMRS:INCLude | command/query

Gets or sets a value indicating whether the PUCCH channel's DMRS is included in EVM calculations and shown in traces

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUCCh:DMRS:INCLude <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUCCh:DMRS:INCLude?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PUCC:DMRS:INCL 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.Pucch.IncludeDmrs

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |