[:SENSe]:TDSCdma:ADVanced:SUBFrame:SYNC | command/query

Gets or sets the subframe synchronization type.

Command Syntax: | [:SENSe]:TDSCdma:ADVanced:SUBFrame:SYNC <value>
<value> | ::= | "Pilot" | "Midamble"
Query Syntax: | [:SENSe]:TDSCdma:ADVanced:SUBFrame:SYNC?
Returns | ::= | "Pilot" | "Midamble"
Remarks: | <none>
Example: |
    :TDSC:ADV:SUBF:SYNC "Pilot"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.SubframeSynchronization Agilent.SA.Vsa.Tdscdma.SubframeSynchronizationType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |