[:SENSe]:LTE:PROFile:PHICh:MIDefinition | command/query

Gets or sets the definition of m(i) to define the specific PHICH configuration for different sub-frames (TDD only).

Command Syntax: | [:SENSe]:LTE:PROFile:PHICh:MIDefinition <value>
<value> | ::= | "Standard211" | "StandardEvolvedTestModel"
Query Syntax: | [:SENSe]:LTE:PROFile:PHICh:MIDefinition?
Returns | ::= | "Standard211" | "StandardEvolvedTestModel"
Remarks: | <none>
Example: |
    :LTE:PROF:PHIC:MID "Standard211"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PhichMIDefinition Agilent.SA.Vsa.Lte.PhichMIDefinitionType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |