[:SENSe]:GSM:TIME:SLOT:OFFSet | command/query

Gets or sets the time slot offset to use when TSC auto detection is disabled.

Command Syntax: | [:SENSe]:GSM:TIME:SLOT:OFFSet <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:GSM:TIME:SLOT:OFFSet?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.GsmEdgeEvolution.Interfaces.MeasurementExtension.TimeslotOffset

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |