[:SENSe]:LTE:ADVanced:EQUalizer:TRAining | command/query

Gets or sets the equalizer training type as being Off or RS-based or RS+Data based.

Command Syntax: | [:SENSe]:LTE:ADVanced:EQUalizer:TRAining <value>
<value> | ::= | "Off" | "Pilots" | "PilotsAndData"
Query Syntax: | [:SENSe]:LTE:ADVanced:EQUalizer:TRAining?
Returns | ::= | "Off" | "Pilots" | "PilotsAndData"
Remarks: | <none>
Example: |
    :LTE:ADV:EQU:TRA "Off"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.EqualizerTraining Agilent.SA.Vsa.Lte.EqualizerTrainingType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |