[:SENSe]:LTE:PROFile:ULINk:USER:PUCCh:ALLocation:OS | command/query

Gets or sets the Orthogonal Sequence for the allocation/channel.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUCCh:ALLocation[1:N]:OS <value>
<value> | ::= | "Zero" | "One" | "Two"
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUCCh:ALLocation[1:N]:OS?
Returns | ::= | "Zero" | "One" | "Two"
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PUCC:ALL:OS "Zero"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.AllocationBase.OS Agilent.SA.Vsa.Lte.OSIndexType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |