[:SENSe]:DDEMod:FILTer:REFerence | command/query

Gets or sets the reference filter applied during the digital demodulation measurement.

Command Syntax: | [:SENSe]:DDEMod:FILTer:REFerence <value>
<value> | ::= | "Rectangular" | "RaisedCosine" | "RootRaisedCosine" | "Gaussian" | "UserDefined" | "IS95Baseband" | "Edge" | "HalfSine" | "RectangularOneSymbolDuration" | "RaisedCosineThreeSymbolDuration" | "ShapedOffsetQpskTGIrig10604"
Query Syntax: | [:SENSe]:DDEMod:FILTer:REFerence?
Returns | ::= | "Rectangular" | "RaisedCosine" | "RootRaisedCosine" | "Gaussian" | "UserDefined" | "IS95Baseband" | "Edge" | "HalfSine" | "RectangularOneSymbolDuration" | "RaisedCosineThreeSymbolDuration" | "ShapedOffsetQpskTGIrig10604"
Remarks: | <none>
Example: |
    :DDEM:FILT:REF "Rectangular"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.ReferenceFilter Agilent.SA.Vsa.DigitalDemod.ReferenceFilter

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |