:INPut:ANALog:COUPling:LIST | command/query

Gets or sets whether input coupling is AC or DC.

Command Syntax: | :INPut:ANALog:COUPling:LIST <couplingArgs>
<couplingArgs> | ::= | Comma separated values of AC | DC
Query Syntax: | :INPut:ANALog:COUPling:LIST?
Returns | ::= | Comma separated values of AC | DC
Remarks: | <none>
Example: |
    :INP:ANAL:COUP:LIST AC,AC
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AnalogChannel.Coupling

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |