:SYSTem:VSA:HARDware:CONFiguration:ANALyzer:ROSCillator:SOURce:TYPE | command/query

Gets or sets a value indicating whether the configuration should lock to the external reference signal or not.

Command Syntax: | :SYSTem:VSA:HARDware:CONFiguration:ANALyzer:ROSCillator:SOURce:TYPE <source>
<source> | ::= | INT | EXT
Query Syntax: | :SYSTem:VSA:HARDware:CONFiguration:ANALyzer:ROSCillator:SOURce:TYPE?
Returns | ::= | INT | EXT
Remarks: | <none>
Example: |
    :SYST:VSA:HARD:CONF:ANAL:ROSC:SOUR:TYPE INT
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.HardwareConfiguration.EnableExternalReferenceLock

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |