[:SENSe]:TDSCdma:TIME:REFerence | command/query

Gets or sets the time reference.

Command Syntax: | [:SENSe]:TDSCdma:TIME:REFerence <value>
<value> | ::= | "DownlinkPilotTimeSlot" | "UplinkPilotTimeSlot" | "TriggerPoint"
Query Syntax: | [:SENSe]:TDSCdma:TIME:REFerence?
Returns | ::= | "DownlinkPilotTimeSlot" | "UplinkPilotTimeSlot" | "TriggerPoint"
Remarks: | <none>
Example: |
    :TDSC:TIME:REF "DownlinkPilotTimeSlot"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.TimeReference Agilent.SA.Vsa.Tdscdma.TimeReferenceType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |