[:SENSe]:TDSCdma:CODE:FORCE | command/query

Gets or sets how the downlink pilot code, uplink pilot code, scramble code and basic midamble code values change when one of them is modified.

Command Syntax: | [:SENSe]:TDSCdma:CODE:FORCE <value>
<value> | ::= | "DownlinkPilot" | "AnyCode"
Query Syntax: | [:SENSe]:TDSCdma:CODE:FORCE?
Returns | ::= | "DownlinkPilot" | "AnyCode"
Remarks: | <none>
Example: |
    :TDSC:CODE:FORCE "DownlinkPilot"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.ForceCodeGroup Agilent.SA.Vsa.Tdscdma.ForceCodeGroupType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |