[:SENSe]:W16E:MIMO:ANTenna:INACtive | command/query

Gets or sets a value indicating whether antenna paths below -30dB in power from the highest power antenna path are shown or blanked on the MIMO traces.

Command Syntax: | [:SENSe]:W16E:MIMO:ANTenna:INACtive <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:W16E:MIMO:ANTenna:INACtive?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :W16E:MIMO:ANT:INAC 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.IsInactiveAntennaPathsIncluded

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |