[:SENSe]:LTE:PROFile:DLINk:USER:COUPling:POWer:BOOSt | command/query

Gets or sets a value indicating whether all the allocations share the same Power Boost.

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:COUPling:POWer:BOOSt <enabled>
<enabled> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:COUPling:POWer:BOOSt?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:DLIN:USER:COUP:POW:BOOS 0
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.Channel.IsPowerBoostCoupled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |