:TRACe:MARKer:ACP:BANDwidth:CHANnel | command/query

Gets or sets the bandwidth for this adjacent channel.

Command Syntax: | :TRACe[1:N]:MARKer:ACP:BANDwidth:CHANnel[1:N] <bandwidth>
<bandwidth> | ::= | Real number
Query Syntax: | :TRACe[1:N]:MARKer:ACP:BANDwidth:CHANnel[1:N]?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AcpAdjacentChannel.BW

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |