[:SENSe]:WCDMa:CHANnel:DESPread:ULINk:MOD | command/query

Gets or sets the modulation for the despread channel in uplink measurements.

Command Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:ULINk:MOD <value>
<value> | ::= | "Bpsk" | "Pam4"
Query Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:ULINk:MOD?
Returns | ::= | "Bpsk" | "Pam4"
Remarks: | <none>
Example: |
    :WCDM:CHAN:DESP:ULIN:MOD "Bpsk"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.UplinkChannelModulation Agilent.SA.Vsa.Wcdma.UplinkChannelModulation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |