[:SENSe]:W16D[:FORMat]:GUARd[:INTerval] | command/query

Gets or sets the guard interval (cyclic prefix) of the signal, as a fraction of the IFFT time length.

Command Syntax: | [:SENSe]:W16D[:FORMat]:GUARd[:INTerval] <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:W16D[:FORMat]:GUARd[:INTerval]?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdm.Interfaces.MeasurementExtension.GuardInterval

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |