[:SENSe]:RFID[:FORMat]:FWD:CODing | command/query

Gets or sets the line coding for forward (Interrogator -> Tag) bursts.

Command Syntax: | [:SENSe]:RFID[:FORMat]:FWD:CODing <value>
<value> | ::= | "None" | "Manchester" | "FM0" | "Miller" | "Miller2" | "Miller4" | "Miller8" | "PieTypeA" | "PieTypeC" | "ModifiedMiller" | "SubcarrierManchester" | "Bpsk1" | "Bpsk2" | "Bpsk4" | "Bpsk8" | "Code1Of4" | "Code1Of256" | "Code15693SingleSubcarrierLowRate" | "Code15693SingleSubcarrierHighRate" | "Code15693DualSubcarrierLowRate" | "Code15693DualSubcarrierHighRate"
Query Syntax: | [:SENSe]:RFID[:FORMat]:FWD:CODing?
Returns | ::= | "None" | "Manchester" | "FM0" | "Miller" | "Miller2" | "Miller4" | "Miller8" | "PieTypeA" | "PieTypeC" | "ModifiedMiller" | "SubcarrierManchester" | "Bpsk1" | "Bpsk2" | "Bpsk4" | "Bpsk8" | "Code1Of4" | "Code1Of256" | "Code15693SingleSubcarrierLowRate" | "Code15693SingleSubcarrierHighRate" | "Code15693DualSubcarrierLowRate" | "Code15693DualSubcarrierHighRate"
Remarks: | <none>
Example: |
    :RFID:FWD:COD "None"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.ForwardLineCoding Agilent.SA.Vsa.Rfid.LineCodeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |