[:SENSe]:LTE:ADVanced:CPLength | command/query

Gets or sets the Cyclic Prefix length mode as being auto-detected, normal or extended.

Command Syntax: | [:SENSe]:LTE:ADVanced:CPLength <value>
<value> | ::= | "Auto" | "Normal" | "Extended"
Query Syntax: | [:SENSe]:LTE:ADVanced:CPLength?
Returns | ::= | "Auto" | "Normal" | "Extended"
Remarks: | <none>
Example: |
    :LTE:ADV:CPL "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.CyclicPrefixLengthMode Agilent.SA.Vsa.Lte.CyclicPrefixLengthModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |