:INPut:ANALog:IMPedance:REFerence:CONNection:LIST | command/query

Gets or sets a value indicating whether the reference impedance follows the connector impedance.

Command Syntax: | :INPut:ANALog:IMPedance:REFerence:CONNection:LIST <cnxArgs>
<cnxArgs> | ::= | Comma separated values of 0 | 1
Query Syntax: | :INPut:ANALog:IMPedance:REFerence:CONNection:LIST?
Returns | ::= | Comma separated values of Integer number
Remarks: | <none>
Example: |
    :INP:ANAL:IMP:REF:CONN:LIST 0,0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AnalogChannel.RefImpedanceIsConnection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |