[:SENSe]:LTE:ADVanced:EVM:WINDow:MODE | command/query

Gets or sets the EVM Window Length mode as being 3GPP standard-defined or custom-defined

Command Syntax: | [:SENSe]:LTE:ADVanced:EVM:WINDow:MODE <value>
<value> | ::= | "Mode3Gpp" | "Custom"
Query Syntax: | [:SENSe]:LTE:ADVanced:EVM:WINDow:MODE?
Returns | ::= | "Mode3Gpp" | "Custom"
Remarks: | <none>
Example: |
    :LTE:ADV:EVM:WIND:MODE "Mode3Gpp"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.EvmWindowLengthMode Agilent.SA.Vsa.Lte.WindowLengthModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |