[:SENSe]:LTE:PROFile:DLINk:USER:ALLocation:POWer:EPRE | command/query

Gets or sets the per-antenna EPRE in dB of the allocation/user.

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:ALLocation[1:N]:POWer:EPRE <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:ALLocation[1:N]:POWer:EPRE?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.AllocationBase.PerAntennaEpre

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |