[:SENSe]:TEDS[:FORMat]:BANDwidth | command/query

Gets or sets a value indicating the channel bandwidth.

Command Syntax: | [:SENSe]:TEDS[:FORMat]:BANDwidth <value>
<value> | ::= | "Bandwidth25Khz" | "Bandwidth50Khz" | "Bandwidth100Khz" | "Bandwidth150Khz"
Query Syntax: | [:SENSe]:TEDS[:FORMat]:BANDwidth?
Returns | ::= | "Bandwidth25Khz" | "Bandwidth50Khz" | "Bandwidth100Khz" | "Bandwidth150Khz"
Remarks: | <none>
Example: |
    :TEDS:BAND "Bandwidth25Khz"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Teds.Interfaces.MeasurementExtension.ChannelBandwidth Agilent.SA.Vsa.Teds.ChannelBandwidth

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |