:INPut:TRIGger:FMASk:RBWMode | command/query

Gets or sets how the ResBW is controlled for the frequency mask trigger.

Command Syntax: | :INPut:TRIGger:FMASk:RBWMode <value>
<value> | ::= | "Auto" | "Manual"
Query Syntax: | :INPut:TRIGger:FMASk:RBWMode?
Returns | ::= | "Auto" | "Manual"
Remarks: | <none>
Example: |
    :INP:TRIG:FMAS:RBWM "Auto"
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.FrequencyMaskTrigger.ResBWMode Agilent.SA.Vsa.FrequencyMaskTriggerResBWMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |