[:SENSe]:LTE:TIME:BOUNdary:STARt | command/query

Gets or sets the analysis start boundary.

Command Syntax: | [:SENSe]:LTE:TIME:BOUNdary:STARt <value>
<value> | ::= | "Frame" | "HalfFrame" | "Subframe" | "Slot"
Query Syntax: | [:SENSe]:LTE:TIME:BOUNdary:STARt?
Returns | ::= | "Frame" | "HalfFrame" | "Subframe" | "Slot"
Remarks: | <none>
Example: |
    :LTE:TIME:BOUN:STAR "Frame"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.AnalysisStartBoundary Agilent.SA.Vsa.Lte.AnalysisBoundaryType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |