:TRACe:GRAPh:COMPensate:PHASe:ERRor:AUTO | command/query

Gets or sets a value indicating whether phase error compensation will use the default filter length.

Command Syntax: | :TRACe[1:N]:GRAPh:COMPensate:PHASe:ERRor:AUTO <value>
<value> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:GRAPh:COMPensate:PHASe:ERRor:AUTO?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:GRAP:COMP:PHAS:ERR:AUTO 0
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Graph.IsPhaseErrorCompensateAuto

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |