:TRACe:MARKer:BANDwidth:SPAN | command/query

Gets or sets the Band Power calculation region.

Command Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:SPAN <bandSpan>
<bandSpan> | ::= | Real number
Query Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:SPAN?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.BandSpan

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |