[:SENSe]:LTE[:FORMat]:DLINk:MIMO[:DECoding] | command/query

Gets or sets the MIMO decoding to apply to channels that have undergone MIMO precoding.

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:MIMO[:DECoding] <value>
<value> | ::= | "Off" | "JointEqualizer" | "ThreeGpp"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:MIMO[:DECoding]?
Returns | ::= | "Off" | "JointEqualizer" | "ThreeGpp"
Remarks: | <none>
Example: |
    :LTE:DLIN:MIMO "Off"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.MimoDecoding Agilent.SA.Vsa.Lte.MimoDecodingType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |