[:SENSe]:LTE:ADVanced:UERS:COMPensate:WEIGht:RI | command/query

Gets or sets a value indicating whether UE-specific RS weights displayed in the UE-specific RS weights table are in Real/Imaginary format

Command Syntax: | [:SENSe]:LTE:ADVanced:UERS:COMPensate:WEIGht:RI <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:ADVanced:UERS:COMPensate:WEIGht:RI?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:ADV:UERS:COMP:WEIG:RI 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsUersWeightsInRealImaginaryEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |