[:SENSe]:TEDS:ANALysis:SUBCarrier:LOCation | command/query

Gets or sets a value indicating the location of the analyzed subcarrier.

Command Syntax: | [:SENSe]:TEDS:ANALysis:SUBCarrier:LOCation <value>
<value> | ::= | "R1" | "R2" | "R3" | "R4" | "R5" | "R6" | "R7" | "R8" | "R9" | "R10" | "R11" | "R12" | "R13" | "R14" | "R15" | "R16" | "R17" | "R18" | "R19" | "R20" | "R21" | "R22" | "R23" | "R24" | "L24" | "L23" | "L22" | "L21" | "L20" | "L19" | "L18" | "L17" | "L16" | "L15" | "L14" | "L13" | "L12" | "L11" | "L10" | "L9" | "L8" | "L7" | "L6" | "L5" | "L4" | "L3" | "L2" | "L1"
Query Syntax: | [:SENSe]:TEDS:ANALysis:SUBCarrier:LOCation?
Returns | ::= | "R1" | "R2" | "R3" | "R4" | "R5" | "R6" | "R7" | "R8" | "R9" | "R10" | "R11" | "R12" | "R13" | "R14" | "R15" | "R16" | "R17" | "R18" | "R19" | "R20" | "R21" | "R22" | "R23" | "R24" | "L24" | "L23" | "L22" | "L21" | "L20" | "L19" | "L18" | "L17" | "L16" | "L15" | "L14" | "L13" | "L12" | "L11" | "L10" | "L9" | "L8" | "L7" | "L6" | "L5" | "L4" | "L3" | "L2" | "L1"
Remarks: | <none>
Example: |
    :TEDS:ANAL:SUBC:LOC "R1"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Teds.Interfaces.MeasurementExtension.AnalysisSubcarrier Agilent.SA.Vsa.Teds.SubcarrierLocation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |