:INPut:ANALog:COUPling | command/query

Gets or sets the input coupling (either AC or DC).

Command Syntax: | :INPut:ANALog:COUPling <coupling>
<coupling> | ::= | AC | DC
Query Syntax: | :INPut:ANALog:COUPling?
Returns | ::= | AC | DC
Remarks: | <none>
Example: |
    :INP:ANAL:COUP AC
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Analog.Coupling

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |