:TRACe:DEMod:ALINe[:VISible] | command/query

Gets or sets a value indicating whether a 2D demodulation trace should have an overlaid average line.

Command Syntax: | :TRACe[1:N]:DEMod:ALINe[:VISible] <value>
<value> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:DEMod:ALINe[:VISible]?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:DEM:ALIN 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.IsDemod2DAverageLineVisible

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |