:TRACe:DATA:STATus | query

Returns the value of the bitflags that make up the MeasurementData.Status property in the .NET Interface.

Query Syntax: | :TRACe[1:N]:DATA:STATus?
Returns | ::= | Integer number
Remarks: | NOTE: The query returns the complete value of all flags. Status flag values:
    None                  (0): Indicates no status messages
    NoData                (1): Indicates no valid data associated with this trace
    Questionable          (2): Indicates data is questionable relative to the current setup.
    Overload              (4): Indicates trace contains an ADC overload.
    Uncalibrated         (16): Indicates that the data in the trace is uncorrected
                               or not fully corrected.
    NoPulse              (64): Indicates a pulse is not found. ("Pulse Not Found"
                               status bit only applies to Digital Modulation
                               Analysis (Option AYA).)
    NoSync              (128): Indicates a sync is not found. ("Sync Not Found"
                               status bit only applies to Digital Modulation Analysis
                               (Option AYA) and LTE analysis (Option BHD or BHE).
    CarrierUnlocked    (1024): Indicates that the hardware is unable to lock to the signal.
    Equalized          (2048): Indicates the digital demodulation equalizer is on.
    Range              (4096): Indicates a PDF or CDF found a sample with a magnitude
                               greater than 100% of the input range.
    AllPoints          (8192): Indicates "Show All Frequency Points" is turned on.
    MeasurementOffset (16384): Indicates the measurement offset parameter is non-zero
                               or the measurment interval parameter is greater than one.
                               Applicable for W-CDMA or cdma2000 measurements.
    ChannelInactive   (32768): Indicates the currently selected channel is not active.
                               Applicable for W-CDMA or cdma2000 measurements.
Version: | 15.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.MeasurementData.Status

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |