[:SENSe]:DDEMod[:FORMat]:MOD | command/query

Gets or sets the digital modulation format used by the signal under test.

Command Syntax: | [:SENSe]:DDEMod[:FORMat]:MOD <value>
<value> | ::= | "Qam16" | "Qam32" | "Qam64" | "Qam256" | "Qpsk" | "DifferentialQpsk" | "Pi4DifferentialQpsk" | "OffsetQpsk" | "Bpsk" | "Psk8" | "Msk" | "Msk2" | "Fsk2" | "Fsk4" | "DvbQam16" | "DvbQam32" | "DvbQam64" | "Vsb8" | "Vsb16" | "Edge" | "Fsk8" | "Fsk16" | "Qam128" | "DifferentialPsk8" | "Qam512" | "Qam1024" | "Apsk16" | "Apsk16Dvb" | "Apsk32" | "Apsk32Dvb" | "DvbQam128" | "DvbQam256" | "Pi8DifferentialPsk8" | "CpmFM" | "Star16Qam" | "Star32Qam" | "CustomApsk" | "ShapedOffsetQpsk" | "Qam2048" | "Qam4096"
Query Syntax: | [:SENSe]:DDEMod[:FORMat]:MOD?
Returns | ::= | "Qam16" | "Qam32" | "Qam64" | "Qam256" | "Qpsk" | "DifferentialQpsk" | "Pi4DifferentialQpsk" | "OffsetQpsk" | "Bpsk" | "Psk8" | "Msk" | "Msk2" | "Fsk2" | "Fsk4" | "DvbQam16" | "DvbQam32" | "DvbQam64" | "Vsb8" | "Vsb16" | "Edge" | "Fsk8" | "Fsk16" | "Qam128" | "DifferentialPsk8" | "Qam512" | "Qam1024" | "Apsk16" | "Apsk16Dvb" | "Apsk32" | "Apsk32Dvb" | "DvbQam128" | "DvbQam256" | "Pi8DifferentialPsk8" | "CpmFM" | "Star16Qam" | "Star32Qam" | "CustomApsk" | "ShapedOffsetQpsk" | "Qam2048" | "Qam4096"
Remarks: | <none>
Example: |
    :DDEM:MOD "Qam16"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.Format Agilent.SA.Vsa.DigitalDemod.Format

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |