[:SENSe]:LTE:PROFile:POWer:AUTO:DCHannel:PBASed | command/query

Gets or sets a value indicating whether DL power levels are auto-detected (only for power-based auto-detection)

Command Syntax: | [:SENSe]:LTE:PROFile:POWer:AUTO:DCHannel:PBASed <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:POWer:AUTO:DCHannel:PBASed?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:POW:AUTO:DCH:PBAS 0
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsPowerLevelAutoDetectedInPowerMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |