[:SENSe]:LTE:ADVanced:EVM:TIMing | command/query

Gets or sets a value indicating whether EVM Minimization of Timing is enabled.

Command Syntax: | [:SENSe]:LTE:ADVanced:EVM:TIMing <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:ADVanced:EVM:TIMing?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:ADV:EVM:TIM 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsTimingIncludedInEvmMinimization

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |