[:SENSe]:LTE:PROFile:DLINk:USER:UERS:TX:PORT | command/query

Gets or sets the antenna port that UE-specific RS is transmitted on for the DL user.

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:UERS:TX:PORT <value>
<value> | ::= | "Port0" | "Port1" | "Port2" | "Port3" | "Port4" | "Port5" | "Port6" | "Port7" | "Port8"
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:UERS:TX:PORT?
Returns | ::= | "Port0" | "Port1" | "Port2" | "Port3" | "Port4" | "Port5" | "Port6" | "Port7" | "Port8"
Remarks: | <none>
Example: |
    :LTE:PROF:DLIN:USER:UERS:TX:PORT "Port0"
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.DownlinkUser.UersTransmitterPortNumber Agilent.SA.Vsa.Lte.AntennaPortType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |