[:SENSe]:LTE:PROFile:MBSFn:SCONfig | command/query

Gets or sets whether each of the 10 subframes is an MBSFN subframe

Command Syntax: | [:SENSe]:LTE:PROFile:MBSFn:SCONfig <isMbsfnSubframe>
<isMbsfnSubframe> | ::= | Comma separated values of 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:MBSFn:SCONfig?
Returns | ::= | Comma separated values of Integer number
Remarks: | <none>
Example: |
    :LTE:PROF:MBSF:SCON 0,1,1,0,0,0,1,0,1,0
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SetMbsfnSubframeConfig

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |