[:SENSe]:EVDO:CHANnel:RACHannel:ACK | command/query

Gets or sets the active channel(s) in the reverse link direction. Used only if Active Channel Detection mode is something other than Auto.

Command Syntax: | [:SENSe]:EVDO:CHANnel:RACHannel:ACK <channelEnabled>
<channelEnabled> | ::= | 0 | 1
Query Syntax: | [:SENSe]:EVDO:CHANnel:RACHannel:ACK?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :EVDO:CHAN:RACH:ACK 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma1xEvdo.Interfaces.MeasurementExtension.ReverseActiveChannel

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |