:TRACe:MARKer:COUPle | command/query

Gets or sets a value indicating whether the marker x-axis position is coupled to the same-numbered marker (by index) on another trace.

Command Syntax: | :TRACe[1:N]:MARKer[1:N]:COUPle <enabled>
<enabled> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:MARKer[1:N]:COUPle?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:MARK:COUP 0
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.IsCouple

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |