[:SENSe]:TEDS:ANALysis:SUBCarrier:MODulation | command/query

Gets or sets a value indicating the modulation format for data subcarriers.

Command Syntax: | [:SENSe]:TEDS:ANALysis:SUBCarrier:MODulation <value>
<value> | ::= | "Qpsk" | "Qam16" | "Qam64"
Query Syntax: | [:SENSe]:TEDS:ANALysis:SUBCarrier:MODulation?
Returns | ::= | "Qpsk" | "Qam16" | "Qam64"
Remarks: | <none>
Example: |
    :TEDS:ANAL:SUBC:MOD "Qpsk"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Teds.Interfaces.MeasurementExtension.DataSubcarrierModulation Agilent.SA.Vsa.Teds.DataSubcarrierModulation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |