[:SENSe]:W16E:MIMO:ANTenna | command/query

Gets or sets the active antenna to use for STC analysis.

Command Syntax: | [:SENSe]:W16E:MIMO:ANTenna <value>
<value> | ::= | "Antenna0" | "Antenna1" | "Antenna2" | "Antenna3"
Query Syntax: | [:SENSe]:W16E:MIMO:ANTenna?
Returns | ::= | "Antenna0" | "Antenna1" | "Antenna2" | "Antenna3"
Remarks: | <none>
Example: |
    :W16E:MIMO:ANT "Antenna0"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.TransmitAntenna Agilent.SA.Vsa.Ieee80216Ofdma.TransmitAntennaType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |