[:SENSe]:LTE:PROFile:ULINk:USER:PUCCh:POWer:BOOSt | command/query

Gets or sets the per-subcarrier power boost in dB for the allocation/channel.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUCCh:POWer:BOOSt <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUCCh:POWer:BOOSt?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.AllocationBase.PowerBoost

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |