[:SENSe]:W16D[:FORMat]:SCARrier:MODulation | command/query

Gets or sets the modulation format for data subcarriers.

Command Syntax: | [:SENSe]:W16D[:FORMat]:SCARrier:MODulation <value>
<value> | ::= | "Qam16" | "Qam64" | "Qpsk" | "Bpsk"
Query Syntax: | [:SENSe]:W16D[:FORMat]:SCARrier:MODulation?
Returns | ::= | "Qam16" | "Qam64" | "Qpsk" | "Bpsk"
Remarks: | <none>
Example: |
    :W16D:SCAR:MOD "Qam16"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdm.Interfaces.MeasurementExtension.DataSubcarrierModulation Agilent.SA.Vsa.Ieee80216Ofdm.DataSubcarrierModulation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |