:TRACe:MARKer:ACP:ENABle:CHANnel | command/query

Gets or sets a value indicating whether this adjacent channel power is calculated.

Command Syntax: | :TRACe[1:N]:MARKer:ACP:ENABle:CHANnel[1:N] <enable>
<enable> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:MARKer:ACP:ENABle:CHANnel[1:N]?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:MARK:ACP:ENAB:CHAN 0
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AcpAdjacentChannel.Enabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |