[:SENSe]:LTE:DECode:DCIFomats | command/query

Gets or sets the DCI Detection Include to be applied, which determines which supported combination of DCI Format 1, 1B, 1D are present within measured signal

Command Syntax: | [:SENSe]:LTE:DECode:DCIFomats <value>
<value> | ::= | "Format1And1B" | "Format1And1D" | "Format1Only" | "Format1BOnly" | "Format1DOnly"
Query Syntax: | [:SENSe]:LTE:DECode:DCIFomats?
Returns | ::= | "Format1And1B" | "Format1And1D" | "Format1Only" | "Format1BOnly" | "Format1DOnly"
Remarks: | <none>
Example: |
    :LTE:DEC:DCIF "Format1And1B"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.DciDetectInclude Agilent.SA.Vsa.Lte.DciDetectIncludeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |